<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.0">
<drawing>
<library>
<packages>
<package name="TS3633-CM1">
</package>
</packages>
<symbols>
<symbol name="TS3633-CM1">
<pin name="VCC" direction="pwr"/>
<pin name="ENV" direction="out"/>
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TS3633-CM1">
<description>Triad’s TS3633-CM1 is a rapid-prototyping solution for creating a SteamVR™ Tracked Object. The TS3633-CM1 is a complete Light-to-Digital Converter on an easy to solder castellated module. The CM1 contains all the circuitry necessary to convert SteamVR Tracking base station infrared light into a digital output that encodes the angle of the sensor from the base station.</description>
<gates>
<gate name="G$1" symbol="TS3633-CM1"/>
</gates>
<devices>
<device name="" package="TS3633-CM1">
<connects>
<connect gate="G$1" pin="ENV" pad="ENV"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
